Samples - Sampling methods

Page / - last modified by TerraIndex TerraIndex on 2021/07/16 15:59

Sampling methods

last modified by TerraIndex TerraIndex

on 2021/07/16 15:59

Table of Contents

The method used to separate large from small grains or particles

Mobile sieving

Sieve means a utensil consisting of a mesh (at intervals of 2mm) held in a frame, used to separate gravel from the fine fraction of soil. For sieving the following is use: each soil sample must be sieved to separate the <2 mm fraction from any gravel or larger detritus (≥2 mm). If the sample contains a large amount of soil (for example, a composite), sieving should be carried out in small batches to prevent soil loss. The sieve should be gently shaken to allow the soil to pass through. The ≥2 mm fraction that does not pass through the sieve should be collected and set aside. If soil aggregates are present in the ≥2 mm fraction after sieving, the crushing and sieving steps should be repeated. The gravel fraction (≥2 mm) from each core or composite sample must be weighed separately and this mass must be recorded.

Raking

Raking is the other method, mostly used for soil with much vegetation or with large particles like gravel and stones. So the parts removed from the soil are at least 2 mm big

References

NPR 5741:2015

Sampling methods

Image	Sampling methods

Contents

Mobile sieving

Raking

References

Sampling methods